:mod:`faulthandler`: On Linux 5.14 and newer, dynamically determine size of
signal handler stack size CPython allocates using ``getauxval(AT_MINSIGSTKSZ)``.
This changes allows for Python extension's request to Linux kernel to use
AMX_TILE instruction set on Sapphire Rapids Xeon processor to succeed,
unblocking use of the ISA in frameworks.
